{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Foglio1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Foglio1","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[]}
[]
[null,"sr",0,"m"]
[null,"sb",1,"m"]
[null,"Ltr",2.2999999999999998,"m"]
[]
[null,"Lunghezza di diffusione trasversale",{"$f":"+C4+2*(C3*0.25+C2*2/3)","v":2.8},"m"]
[null,"Lunghezza di diffusione longitudinale",{"$f":"6.4+(C3/4)*2","v":6.9},"m"]
[]
[null,"Carico concentrato LM71"]
[null,"Qv",1000,"kN","carico concentrato"]
[null,"B",{"$f":"C6","v":2.8},"m","larghezza di diffusione"]
[null,"L",{"$f":"+C7","v":6.9},"m","lunghezza di diffusione"]
[null,"e",0.08,"m","eccentricità convenzionale"]
[null,"eg",0,"m","eccentricità geometrica"]
[null,"etot=e+eg",{"$f":"+C13+C14","v":0.08},"m","eccentricità totale"]
[null,"M=Qv x etot",{"$f":"+C10*C15","v":80},"kNm","Momento rispetto al punto M"]
[null,"a",1.1000000000000001,"-","coef. Di adattamento"]
[null,"[sA=Qv/(BxL)-Mx6(LxB2)] x a",{"$f":"(+C10/(C11*C12)-C16*6/(C12*C11^2))*C17","v":47.175391895888794},"kN/m2","Carico nel punto A"]
[null,"[sB=Qv/(BxL)+Mx6(LxB2)] x a",{"$f":"(+C10/(C11*C12)+C16*6/(C12*C11^2))*C17","v":66.696243714877269},"kN/m2","Carico nel punto B"]
[]
[null,"Carico distribuito LM71"]
[null,"Qv",80,"kN/m","carico concentrato"]
[null,"B",{"$f":"C6","v":2.8},"m","larghezza di diffusione"]
[null,"L",1,"m","lunghezza di diffusione"]
[null,"e",0.08,"m","eccentricità convenzionale"]
[null,"eg",0,"m","eccentricità geometrica"]
[null,"etot=e+eg",{"$f":"+C25+C26","v":0.08},"m","eccentricità totale"]
[null,"M=Qv x etot",{"$f":"+C22*C27","v":6.4},"kNm","Momento rispetto al punto M"]
[null,"a",1.1000000000000001,"-","coef. Di adattamento"]
[null,"[sA=Qv/(Bx1)-Mx6(1xB2)] x a",{"$f":"(+C22/(C23)-C28*6/(C23^2))*C29","v":26.040816326530614},"kN/m2","Carico nel punto A"]
[null,"[sB=Qv/(Bx1)+Mx6(1xB2)] x a",{"$f":"(+C22/(C23)+C28*6/(C23^2))*C29","v":36.816326530612251},"kN/m2","Carico nel punto B"]
[]
[null,"Carico distribuito SW2"]
[null,"Qv",150,"kN/m","carico concentrato"]
[null,"B",{"$f":"C6","v":2.8},"m","larghezza di diffusione"]
[null,"L",1,"m","lunghezza di diffusione"]
[null,"e",0,"m","eccentricità convenzionale"]
[null,"eg",0,"m","eccentricità geometrica"]
[null,"etot=e+eg",{"$f":"+C37+C38","v":0},"m","eccentricità totale"]
[null,"M=Qv x etot",{"$f":"+C34*C39","v":0},"kNm","Momento rispetto al punto M"]
[null,"sA=Qv/(Bx1)-Mx6(1xB2)",{"$f":"+C34/(C35)-C40*6/(C35^2)","v":53.571428571428577},"kN/m2","Carico nel punto A"]
[null,"sB=Qv/(Bx1)+Mx6(1xB2)",{"$f":"+C34/(C35)+C40*6/(C35^2)","v":53.571428571428577},"kN/m2","Carico nel punto B"]